<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="159.1" y2="0" width="0" layer="20"/>
<wire x1="159.1" y1="0" x2="159.1" y2="88.4" width="0" layer="20"/>
<wire x1="159.1" y1="88.4" x2="0" y2="88.4" width="0" layer="20"/>
<wire x1="0" y1="88.4" x2="0" y2="0" width="0" layer="20"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>ASMO Board</text>
<text>Rev: 2.1</text>
<text>19.01.2021</text>
<text>19.01.2021 Rev: 2.1</text>
<text>3 5</text>
<text>I</text>
<text>DA-VREF</text>
<text>HW Flow Control</text>
<text>power CANbus</text>
<text>CAN Term</text>
<text>I</text>
<text>7Seg En</text>
<text>LEDs</text>
<text>Buttons</text>
<text>| +</text>
<text>| +</text>
<text>CAN Speed</text>
<text>High   Std</text>
<text>Ethernet</text>
<text>USB</text>
<text>SE-Interface</text>
<text>SD-Card</text>
<text>PWR</text>
<text>CAN1</text>
<text>CAN2</text>
<text>CAN3</text>
<text>LO</text>
<text>GND</text>
<text>VCC</text>
<text>HI</text>
<text>SD-Card</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="L2825P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
precision wire wound</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="153CLV-0405">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="L3225P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
precision wire wound</description>
</package>
</packages>
</library>
<library name="jumper">
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-panduit">
<packages>
<package name="057-020-1">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
series 057 contact pc board low profile headers&lt;p&gt;
straight</description>
</package>
</packages>
</library>
<library name="mcp120-130">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-omron">
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-amp">
<packages>
<package name="215877-4">
<description>&lt;b&gt;Modular Jack&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-wago-508">
<packages>
<package name="W237-4P">
<description>&lt;b&gt;WAGO SREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="microchip_can">
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
 150-mil body, package type SN</description>
</package>
</packages>
</library>
<library name="maxim">
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="con-subd">
<packages>
<package name="F09HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SmartECLA">
<packages>
<package name="TSSOP16">
</package>
<package name="HD15H">
</package>
<package name="AMP_227161">
<description>&lt;b&gt;JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC&lt;/b&gt;&lt;p&gt;
Source: amp_227161.pdf</description>
</package>
<package name="ML20L">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="SOD80C">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="con-ml">
<packages>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rectifier">
<packages>
<package name="RB1A">
<description>&lt;b&gt;RECTIFIER&lt;/b&gt;&lt;p&gt;
1 A</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED-0603-TTW">
<description>&lt;b&gt;CHIPLED-0603&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="discrete">
<packages>
<package name="RS-2,5">
<description>&lt;b&gt;Resistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-dil">
<packages>
<package name="A1353HEX">
<description>&lt;b&gt;DIL/CODE SWITCH&lt;/b&gt;&lt;p&gt;
&lt;p&gt;
distributor Buerklin, 17G482</description>
</package>
</packages>
</library>
<library name="maxim-10">
<packages>
<package name="SO24W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AA</description>
</package>
</packages>
</library>
<library name="led-7-segment">
<packages>
<package name="S4301B">
<description>&lt;b&gt;Single Digit LED Numeric Display&lt;/b&gt;&lt;p&gt;
Source: LITEON .. S4301B.pdf</description>
</package>
</packages>
</library>
<library name="con-yamaichi">
<packages>
<package name="FPS009-3000">
<description>&lt;b&gt;SD Card and MMC Reader (Manual Insertion)&lt;/b&gt;&lt;p&gt;
Source: http://www.yamaichi.de/pdf/c_fps009_3000.pdf</description>
</package>
</packages>
</library>
<library name="con-conrad2">
<packages>
<package name="733989-5">
<description>&lt;b&gt;FEMALE PRINT CONNECTOR&lt;/b&gt;&lt;p&gt;
1.1 mm, FUK HING Industries, distributor Conrad</description>
</package>
</packages>
</library>
<library name="inductors">
<packages>
<package name="BNX002">
<description>&lt;b&gt;FILTER&lt;/b&gt;&lt;p&gt;
manufacturer Murata</description>
</package>
</packages>
</library>
<library name="wuerth-elektronik">
<packages>
<package name="WE-CNSW_1206">
<description>SMD Common Mode Noise Suppressor</description>
</package>
</packages>
</library>
<library name="STM32F767ZGT6">
<packages>
<package name="QFP50P2200X2200X160-144N">
</package>
</packages>
</library>
<library name="USBLC6-4SC6">
<packages>
<package name="SOT95P280X145-6N">
<description>&lt;b&gt;SOT-23 (6)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="H1102NLT">
<packages>
<package name="XFMR_H1102NLT">
</package>
</packages>
</library>
<library name="LANCHIP">
<packages>
<package name="QFN50P400X400X100-25N">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SM49">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="SM77H">
<description>&lt;b&gt;3.3V CMOS Clock Oscillator&lt;/b&gt;&lt;p&gt;
Source: www.pletronics.com .. sm77h%203.3v.pdf</description>
</package>
</packages>
</library>
<library name="STMPS2151MTR">
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
<library name="ESDA6V1BC6">
<packages>
<package name="SOT95P280X145-6N">
</package>
</packages>
</library>
<library name="jump-0r-smd">
<description>Soldering jumper and bridges</description>
<packages>
<package name="A0R-JMP">
<description>&lt;b&gt;0R Jumper Variant A&lt;/b&gt;&lt;p&gt;
chip 0805</description>
</package>
</packages>
</library>
<library name="rj45_ixi">
<packages>
<package name="RJ45">
</package>
</packages>
</library>
<library name="REF5025AIDG4">
<packages>
<package name="SOIC127P599X175-8N">
</package>
</packages>
</library>
<library name="crystal-geyer_V1_0">
<description>&lt;BR&gt;&lt;big&gt;&lt;b&gt;GEYER ELECTRONIC --- Your producer for quartz crystals and oscillators&lt;/B&gt;&lt;/big&gt;&lt;br&gt;&lt;Hr&gt;

Version 1.0, 07.06.2016
&lt;hr&gt;
&lt;BR&gt;&lt;BR&gt; 

&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;GEYER ELECTRONIC e.K.&lt;/b&gt;&lt;br&gt;


Lochhamer Schlag 5&lt;br&gt;
D-82166 Gräfelfing/München&lt;br&gt;
&lt;br&gt;
Tel:   +49 89 546868-0&lt;br&gt;
Fax: +49 89 546868-90 für Batterien und Ladetechnik&lt;br&gt;
Fax: +49 89 546868-91 für Quarzprodukte&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.geyer-electronic.de"&gt;http://www.geyer-electronic.de&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:info@geyer-electronic.de"&gt;info@geyer-electronic.de&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor Geyer-Electronic does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Copyright: Geyer-Electronic</description>
<packages>
<package name="6.0X3.5_2">
<description>2 Pad</description>
</package>
</packages>
</library>
<library name="Amphenol_MicroUSB">
<packages>
<package name="MICRO_USB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JTAG" library="con-panduit" package="057-020-1" value="057-020-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="mcp120-130" package="SOT23" value="MCP120/130">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-omron" package="B3F-10XX" value="RESET">
<attribute name="MF" value=""/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="POPULARITY" value="72"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0805" value="330">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ_2" value="STD/HS">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="7"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-amp" package="215877-4" value="RJ1">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="con-amp" package="215877-4" value="RJ2">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X02" value="offen">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="98"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="con-wago-508" package="W237-4P" value="CON">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="120">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="microchip_can" package="SO-08" value="MCP2551SN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="maxim" package="SO16" value="MAX3232CSE">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MAX3232CSE"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9725490"/>
<attribute name="OC_NEWARK" value="90C2890"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="jumper" package="JP1" value="HW_FLOW_CONTROL">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="61"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="330">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-subd" package="F09HP" value="RS232">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0805" value="0">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0805" value="2k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0805" value="33k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0805" value="33k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="L2825P" value="470nH">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="L"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl" package="C0805K" value="4,7uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SmartECLA" package="TSSOP16" value="AD5317">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ_2" value="V_REF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="7"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SmartECLA" package="TSSOP16" value="AD7924">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rcl" package="153CLV-0405" value="10µ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl" package="153CLV-0405" value="10µ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rcl" package="153CLV-0405" value="10µ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="DSUB_SCHNITTSTELLE" library="SmartECLA" package="HD15H" value="DSUB-SIGNALE">
<attribute name="VALUE"/>
</element>
<element name="DISPLAY" library="con-ml" package="ML10" value="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D12" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D15" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D16" library="diode" package="SOT23" value="BAS40-04">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="B1" library="rectifier" package="RB1A" value="0">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="12"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="linear" package="TO220H" value="7805T">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="35"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="rcl" package="153CLV-0405" value="10u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="linear" package="TO220H" value="LM33 CV">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="35"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="rcl" package="153CLV-0405" value="10u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0805" value="1800">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0805" value="820">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIPLED-0603-TTW" value="5V">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED-0603-TTW" value="3.3V">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X02" value="offen">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="98"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="TR1" library="discrete" package="RS-2,5" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="switch-dil" package="A1353HEX" value="Default 0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="maxim-10" package="SO24W" value="MAX7221CWG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0805" value="27k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led-7-segment" package="S4301B" value="S4301B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led-7-segment" package="S4301B" value="S4301B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led-7-segment" package="S4301B" value="S4301B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led-7-segment" package="S4301B" value="S4301B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="jumper" package="JP2" value="7Seg Disable">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="34"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="pinhead" package="2X04" value="Buttons">
<attribute name="POPULARITY" value="47"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="led" package="LED3MM" value="3,3V">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="97"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0805" value="680">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="LED3MM" value="5V">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="97"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R0805" value="1500">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-yamaichi" package="FPS009-3000" value="FPS009-3000">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="con-conrad2" package="733989-5" value="9-12V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="153CLV-0405" value="10u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C53" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="inductors" package="BNX002" value="BNX002">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="VALUE"/>
</element>
<element name="L5" library="wuerth-elektronik" package="WE-CNSW_1206" value="Würth 744232102">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L6" library="wuerth-elektronik" package="WE-CNSW_1206" value="Würth 744232102">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L7" library="wuerth-elektronik" package="WE-CNSW_1206" value="Würth 744232102">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="diode" package="SOD80C" value="5,6V">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D14" library="diode" package="SOD80C" value="3,9V">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="D17" library="diode" package="SOT23" value="DZ23C36-7-F">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="D18" library="diode" package="SOT23" value="DZ23C36-7-F">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="C61" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C59" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="L8" library="rcl" package="L3225P" value="2.2kOhm@100MHz">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="L"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="rcl" package="L3225P" value="2.2kOhm@100MHz">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="L"/>
<attribute name="VALUE"/>
</element>
<element name="C60" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C57" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C58" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="X5" library="SmartECLA" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="VALUE"/>
</element>
<element name="X6" library="SmartECLA" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="VALUE"/>
</element>
<element name="X7" library="SmartECLA" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="VALUE"/>
</element>
<element name="X8" library="SmartECLA" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="VALUE"/>
</element>
<element name="X9" library="SmartECLA" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="VALUE"/>
</element>
<element name="X10" library="SmartECLA" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="VALUE"/>
</element>
<element name="X11" library="SmartECLA" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="VALUE"/>
</element>
<element name="X12" library="SmartECLA" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="rcl" package="153CLV-0405" value="10µ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="pinhead" package="2X04" value="LEDs">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="47"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="rcl" package="R0805" value="180">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="rcl" package="R0805" value="180">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="rcl" package="R0805" value="180">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="rcl" package="R0805" value="180">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="D19" library="diode" package="SOD80C" value="5,6V">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="STM32F767ZGT6" package="QFP50P2200X2200X160-144N" value="STM32F767ZIT6">
<attribute name="AVAILABILITY" value="Warning"/>
<attribute name="DESCRIPTION" value=" ARM® Cortex®-M7 STM32F7 Microcontroller IC 32-Bit 216MHz 1MB (1M x 8) FLASH 144-LQFP (20x20) "/>
<attribute name="DIGIKEY-PURCHASE-URL" value="https://snapeda.com/shop?store=DigiKey&amp;id=785612"/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=785612"/>
<attribute name="MP" value="STM32F767ZGT6"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="LQFP-144 STMicroelectronics"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="USBLC6-4SC6" package="SOT95P280X145-6N" value="USBLC6-4SC6">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" 17V Clamp 5A (8/20µs) Ipp Tvs Diode Surface Mount SOT-23-6 "/>
<attribute name="DIGIKEY-PURCHASE-URL" value="https://snapeda.com/shop?store=DigiKey&amp;id=562356"/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=562356"/>
<attribute name="MP" value="USBLC6-4SC6"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-6 STMicroelectronics"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="H1102NLT" package="XFMR_H1102NLT" value="H1102NLT">
<attribute name="ARROW_ELECTRONICS-PURCHASE-URL" value="https://snapeda.com/shop?store=Arrow+Electronics&amp;id=78695"/>
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" Isolation and Data Interface (Encapsulated) Pulse Transformer 1:1 Transmitter, 1:1 Receiver Surface Mount "/>
<attribute name="DIGIKEY-PURCHASE-URL" value="https://snapeda.com/shop?store=DigiKey&amp;id=78695"/>
<attribute name="MF" value="Pulse Electronics"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=78695"/>
<attribute name="MP" value="H1102NL"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-16 Pulse"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="LANCHIP" package="QFN50P400X400X100-25N" value="LANCHIP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R64" library="rcl" package="R0805" value="12k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R68" library="rcl" package="R0805" value="1,5k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R69" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R70" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R71" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R72" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R73" library="rcl" package="R0805" value="47">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R74" library="rcl" package="R0805" value="47">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R75" library="rcl" package="R0805" value="47">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R76" library="rcl" package="R0805" value="47">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C76" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C77" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C79" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C80" library="rcl" package="C0805K" value="1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C81" library="rcl" package="C0805K" value="470pF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C82" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C83" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R77" library="rcl" package="R0805" value="75">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R78" library="rcl" package="R0805" value="75">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R79" library="rcl" package="R0805" value="75">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R80" library="rcl" package="R0805" value="75">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C84" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="L10BEAD" library="rcl" package="L2825P" value="470nH">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="L"/>
<attribute name="VALUE"/>
</element>
<element name="C65" library="rcl" package="153CLV-0405" value="10u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R49" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="rcl" package="R0805" value="33">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="rcl" package="R0805" value="33">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C62" library="rcl" package="C0805K" value="18pF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C63" library="rcl" package="C0805K" value="18pF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="rcl" package="R0805" value="33R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="rcl" package="R0805" value="33">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C64" library="rcl" package="C0805K" value="1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="STMPS2151MTR" package="SOIC127P600X175-8N" value="STMPS2151MTR">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" Power Switch/Driver 1:1 N-Channel 500mA 8-SO "/>
<attribute name="DIGIKEY-PURCHASE-URL" value="https://snapeda.com/shop?store=DigiKey&amp;id=271634"/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=271634"/>
<attribute name="MP" value="STMPS2151MTR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-8 STMicroelectronics"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="D20" library="ESDA6V1BC6" package="SOT95P280X145-6N" value="ESDA6V1BC6">
<attribute name="AVAILABILITY" value="Warning"/>
<attribute name="DESCRIPTION" value=" Clamp Ipp Tvs Diode Surface Mount SOT-23-6 "/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=308145"/>
<attribute name="MP" value="ESDA6V1BC6"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-6 STMicroelectronics"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C66" library="rcl" package="153CLV-0405" value="4.7uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="Q2-RTC" library="crystal" package="SM49" value="32.768 kHz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="C67" library="rcl" package="C0805K" value="2pF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C68" library="rcl" package="C0805K" value="2pF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="L10BEAD1" library="rcl" package="L2825P" value="470nH">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="L"/>
<attribute name="VALUE"/>
</element>
<element name="C69" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C70" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C73" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C74" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C75" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C78" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C87" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C88" library="rcl" package="C0805K" value="1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C89" library="rcl" package="C0805K" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C90" library="rcl" package="C0805K" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="JMP1" library="jump-0r-smd" package="A0R-JMP" value="0R-JUMPA">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="rj45_ixi" package="RJ45" value="RJ45">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0805K" value="1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0805K" value="4,7uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="REF5025AIDG4" package="SOIC127P599X175-8N" value="REF5025AIDG4">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" 2.5-V, 3-Vpp/V noise, 3-ppm/C drift precision series voltage reference 8-SOIC -40 to 125 "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="REF5025AIDG4"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-8 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/REF5025AIDG4/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="153CLV-0405" value="22u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="153CLV-0405" value="10µ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="SV5" library="SmartECLA" package="ML20L" value="C1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="8MHZ" library="crystal" package="SM77H" value="SM77H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="crystal-geyer_V1_0" package="6.0X3.5_2" value="25Mhz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0805K" value="10n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="52"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="Amphenol_MicroUSB" package="MICRO_USB" value="10104110-0001LF">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" USB - micro B USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle "/>
<attribute name="MF" value="Amphenol ICC"/>
<attribute name="MP" value="10104110-0001LF"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/10104110-0001LF/?ref=eda"/>
</element>
<element name="R48" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="86"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JTAG" pad="20"/>
<contactref element="JTAG" pad="18"/>
<contactref element="JTAG" pad="16"/>
<contactref element="JTAG" pad="14"/>
<contactref element="JTAG" pad="12"/>
<contactref element="JTAG" pad="10"/>
<contactref element="JTAG" pad="8"/>
<contactref element="JTAG" pad="6"/>
<contactref element="JTAG" pad="4"/>
<contactref element="IC2" pad="3"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="6"/>
<contactref element="X3" pad="4"/>
<contactref element="IC3" pad="15"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C27" pad="1"/>
<contactref element="X2" pad="5"/>
<contactref element="R15" pad="2"/>
<contactref element="U$1" pad="12"/>
<contactref element="U$1" pad="9"/>
<contactref element="C33" pad="-"/>
<contactref element="DSUB_SCHNITTSTELLE" pad="GND"/>
<contactref element="DISPLAY" pad="2"/>
<contactref element="D7" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="D15" pad="1"/>
<contactref element="D16" pad="1"/>
<contactref element="D13" pad="1"/>
<contactref element="D12" pad="1"/>
<contactref element="D11" pad="1"/>
<contactref element="D10" pad="1"/>
<contactref element="D8" pad="1"/>
<contactref element="D9" pad="1"/>
<contactref element="B1" pad="-"/>
<contactref element="IC5" pad="2"/>
<contactref element="C42" pad="-"/>
<contactref element="C44" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="IC4" pad="2"/>
<contactref element="C39" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="IC6" pad="9"/>
<contactref element="IC6" pad="4"/>
<contactref element="R24" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="C46" pad="2"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP7" pad="3"/>
<contactref element="JP7" pad="5"/>
<contactref element="JP7" pad="7"/>
<contactref element="R30" pad="1"/>
<contactref element="R31" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="6"/>
<contactref element="C5" pad="-"/>
<contactref element="C53" pad="1"/>
<contactref element="C52" pad="1"/>
<contactref element="C54" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="C41" pad="-"/>
<contactref element="D5" pad="A"/>
<contactref element="D14" pad="A"/>
<contactref element="D17" pad="1"/>
<contactref element="D18" pad="2"/>
<contactref element="SJ1" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="C32" pad="1"/>
<contactref element="C59" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="C60" pad="2"/>
<contactref element="C56" pad="2"/>
<contactref element="C57" pad="2"/>
<contactref element="C58" pad="1"/>
<contactref element="C38" pad="-"/>
<contactref element="R40" pad="1"/>
<contactref element="R43" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="C82" pad="2"/>
<contactref element="C83" pad="2"/>
<contactref element="C76" pad="2"/>
<contactref element="C77" pad="2"/>
<contactref element="U$3" pad="25"/>
<contactref element="C79" pad="2"/>
<contactref element="C80" pad="2"/>
<contactref element="C81" pad="2"/>
<contactref element="R64" pad="1"/>
<contactref element="C65" pad="-"/>
<contactref element="C84" pad="2"/>
<contactref element="R49" pad="2"/>
<contactref element="C62" pad="1"/>
<contactref element="C63" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U4" pad="1"/>
<contactref element="D20" pad="2"/>
<contactref element="D20" pad="5"/>
<contactref element="R45" pad="2"/>
<contactref element="C66" pad="-"/>
<contactref element="C67" pad="2"/>
<contactref element="C68" pad="2"/>
<contactref element="U2" pad="107"/>
<contactref element="U2" pad="94"/>
<contactref element="U2" pad="120"/>
<contactref element="U2" pad="61"/>
<contactref element="U2" pad="51"/>
<contactref element="U2" pad="83"/>
<contactref element="U2" pad="16"/>
<contactref element="U2" pad="38"/>
<contactref element="U2" pad="130"/>
<contactref element="C78" pad="2"/>
<contactref element="C69" pad="2"/>
<contactref element="C70" pad="2"/>
<contactref element="C73" pad="2"/>
<contactref element="C74" pad="2"/>
<contactref element="C75" pad="2"/>
<contactref element="C87" pad="2"/>
<contactref element="C88" pad="2"/>
<contactref element="C89" pad="2"/>
<contactref element="C90" pad="2"/>
<contactref element="R53" pad="2"/>
<contactref element="JMP1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R47" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C64" pad="2"/>
<contactref element="U$5" pad="GND1"/>
<contactref element="U$5" pad="GND2"/>
<contactref element="8MHZ" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="J4" pad="5"/>
<contactref element="J4" pad="GND"/>
<contactref element="R54" pad="1"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="JTAG" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="JTAG" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C22" pad="2"/>
<contactref element="IC3" pad="16"/>
<contactref element="C27" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="U$2" pad="15"/>
<contactref element="C33" pad="+"/>
<contactref element="SJ2" pad="3"/>
<contactref element="DISPLAY" pad="1"/>
<contactref element="IC4" pad="3"/>
<contactref element="C40" pad="2"/>
<contactref element="LED1" pad="A@1"/>
<contactref element="DSUB_SCHNITTSTELLE" pad="+3.3V"/>
<contactref element="TR1" pad="1"/>
<contactref element="S2" pad="C"/>
<contactref element="R29" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="LED7" pad="A"/>
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C5" pad="+"/>
<contactref element="D14" pad="C"/>
<contactref element="C32" pad="2"/>
<contactref element="C58" pad="2"/>
<contactref element="U$3" pad="9"/>
<contactref element="C79" pad="1"/>
<contactref element="L10BEAD" pad="1"/>
<contactref element="U2" pad="39"/>
<contactref element="U2" pad="72"/>
<contactref element="U2" pad="30"/>
<contactref element="U2" pad="108"/>
<contactref element="U2" pad="84"/>
<contactref element="U2" pad="131"/>
<contactref element="U2" pad="52"/>
<contactref element="U2" pad="17"/>
<contactref element="U2" pad="144"/>
<contactref element="U2" pad="62"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="95"/>
<contactref element="L10BEAD1" pad="1"/>
<contactref element="C69" pad="1"/>
<contactref element="C70" pad="1"/>
<contactref element="C73" pad="1"/>
<contactref element="C78" pad="1"/>
<contactref element="C74" pad="1"/>
<contactref element="C75" pad="1"/>
<contactref element="C88" pad="1"/>
<contactref element="JMP1" pad="1"/>
<contactref element="U2" pad="121"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R70" pad="1"/>
<contactref element="R71" pad="1"/>
<contactref element="R72" pad="1"/>
<contactref element="R68" pad="2"/>
<contactref element="R69" pad="2"/>
<contactref element="8MHZ" pad="1"/>
<contactref element="8MHZ" pad="4"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="JTAG" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="TDI">
<contactref element="JTAG" pad="5"/>
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="110"/>
</signal>
<signal name="TMS">
<contactref element="JTAG" pad="7"/>
<contactref element="R4" pad="1"/>
<contactref element="U2" pad="105"/>
</signal>
<signal name="TCK">
<contactref element="JTAG" pad="9"/>
<contactref element="R5" pad="1"/>
<contactref element="U2" pad="109"/>
</signal>
<signal name="TDO">
<contactref element="JTAG" pad="13"/>
<contactref element="U2" pad="133"/>
</signal>
<signal name="NRST">
<contactref element="JTAG" pad="15"/>
<contactref element="C21" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="U2" pad="25"/>
<contactref element="U2" pad="134"/>
<contactref element="U$3" pad="15"/>
</signal>
<signal name="N$9">
<contactref element="R8" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="CANRX">
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="114"/>
</signal>
<signal name="CANTX">
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="115"/>
</signal>
<signal name="N$7">
<contactref element="SJ1" pad="2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="CANLOW">
<contactref element="R10" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="L6" pad="1"/>
<contactref element="L7" pad="1"/>
<contactref element="D18" pad="1"/>
<contactref element="L5" pad="4"/>
</signal>
<signal name="CANHIGH">
<contactref element="JP5" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="L6" pad="4"/>
<contactref element="L7" pad="4"/>
<contactref element="D17" pad="2"/>
<contactref element="L5" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="DSUB_SCHNITTSTELLE" pad="+5V"/>
<contactref element="D7" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="IC5" pad="3"/>
<contactref element="C44" pad="2"/>
<contactref element="C41" pad="+"/>
<contactref element="LED3" pad="A@1"/>
<contactref element="JP4" pad="1"/>
<contactref element="D15" pad="2"/>
<contactref element="D16" pad="2"/>
<contactref element="D8" pad="2"/>
<contactref element="D10" pad="2"/>
<contactref element="D11" pad="2"/>
<contactref element="D12" pad="2"/>
<contactref element="D13" pad="2"/>
<contactref element="D9" pad="2"/>
<contactref element="IC6" pad="19"/>
<contactref element="R25" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="LED8" pad="A"/>
<contactref element="R36" pad="1"/>
<contactref element="D5" pad="C"/>
<contactref element="SJ1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C59" pad="1"/>
<contactref element="L8" pad="2"/>
<contactref element="C38" pad="+"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="JP5" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC3" pad="2"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="C24" pad="1"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="N$14">
<contactref element="C26" pad="2"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="IC3" pad="5"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="C25" pad="1"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="IC3" pad="1"/>
<contactref element="C25" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="IC3" pad="9"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R9" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="CTS">
<contactref element="R9" pad="1"/>
<contactref element="U2" pad="117"/>
</signal>
<signal name="RXD">
<contactref element="IC3" pad="12"/>
<contactref element="U2" pad="122"/>
</signal>
<signal name="RTS">
<contactref element="IC3" pad="10"/>
<contactref element="U2" pad="118"/>
</signal>
<signal name="TXD">
<contactref element="IC3" pad="11"/>
<contactref element="U2" pad="119"/>
</signal>
<signal name="N$18">
<contactref element="X2" pad="2"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="N$19">
<contactref element="X2" pad="3"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="N$20">
<contactref element="X2" pad="7"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="N$22">
<contactref element="IC3" pad="7"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R11" pad="1"/>
<contactref element="X2" pad="8"/>
</signal>
<signal name="CS_MMC">
<contactref element="X1" pad="1"/>
<contactref element="U2" pad="48"/>
</signal>
<signal name="SCK0">
<contactref element="DISPLAY" pad="9"/>
<contactref element="X1" pad="5"/>
<contactref element="U2" pad="41"/>
</signal>
<signal name="MOSI0">
<contactref element="DISPLAY" pad="8"/>
<contactref element="X1" pad="2"/>
<contactref element="U2" pad="135"/>
</signal>
<signal name="MISO0">
<contactref element="DISPLAY" pad="7"/>
<contactref element="X1" pad="7"/>
<contactref element="R12" pad="2"/>
<contactref element="U2" pad="124"/>
</signal>
<signal name="CD_MMC">
<contactref element="X1" pad="DETECT"/>
<contactref element="R17" pad="2"/>
<contactref element="U2" pad="47"/>
</signal>
<signal name="WP_MMC">
<contactref element="X1" pad="WRITE_PROT"/>
<contactref element="R16" pad="2"/>
<contactref element="U2" pad="46"/>
</signal>
<signal name="VDD">
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="10"/>
<contactref element="U$1" pad="1"/>
<contactref element="SJ2" pad="2"/>
<contactref element="C35" pad="+"/>
<contactref element="C29" pad="2"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="MOSI1">
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="13"/>
<contactref element="DSUB_SCHNITTSTELLE" pad="MOSI"/>
<contactref element="D16" pad="3"/>
<contactref element="IC6" pad="1"/>
<contactref element="U2" pad="76"/>
</signal>
<signal name="OUT1">
<contactref element="U$1" pad="4"/>
<contactref element="X9" pad="1"/>
</signal>
<signal name="OUT3">
<contactref element="U$1" pad="6"/>
<contactref element="X11" pad="1"/>
</signal>
<signal name="IN1">
<contactref element="U$2" pad="12"/>
<contactref element="D3" pad="3"/>
<contactref element="R32" pad="2"/>
<contactref element="C61" pad="1"/>
</signal>
<signal name="IN2">
<contactref element="U$2" pad="11"/>
<contactref element="D2" pad="3"/>
<contactref element="R33" pad="2"/>
<contactref element="C48" pad="1"/>
</signal>
<signal name="IN3">
<contactref element="U$2" pad="10"/>
<contactref element="D1" pad="3"/>
<contactref element="R35" pad="2"/>
<contactref element="C49" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="U$1" pad="11"/>
<contactref element="X12" pad="1"/>
</signal>
<signal name="SCK1">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="14"/>
<contactref element="DSUB_SCHNITTSTELLE" pad="SCK"/>
<contactref element="D9" pad="3"/>
<contactref element="IC6" pad="13"/>
<contactref element="U2" pad="69"/>
</signal>
<signal name="CS_ADC">
<contactref element="U$2" pad="3"/>
<contactref element="U2" pad="139"/>
</signal>
<signal name="N$31">
<contactref element="U$2" pad="7"/>
<contactref element="C30" pad="1"/>
<contactref element="U5" pad="6"/>
<contactref element="C6" pad="+"/>
</signal>
<signal name="MISO1">
<contactref element="U$2" pad="14"/>
<contactref element="U$1" pad="16"/>
<contactref element="DSUB_SCHNITTSTELLE" pad="MISO"/>
<contactref element="D15" pad="3"/>
<contactref element="U2" pad="75"/>
</signal>
<signal name="VIN3">
<contactref element="U$2" pad="9"/>
<contactref element="D4" pad="3"/>
<contactref element="R34" pad="2"/>
<contactref element="C50" pad="2"/>
</signal>
<signal name="CS_DAC">
<contactref element="U$1" pad="15"/>
<contactref element="U2" pad="137"/>
</signal>
<signal name="SIGNAL3_DSUB">
<contactref element="D11" pad="3"/>
<contactref element="R37" pad="1"/>
<contactref element="C57" pad="1"/>
<contactref element="U2" pad="34"/>
</signal>
<signal name="SIGNAL1_DSUB">
<contactref element="D13" pad="3"/>
<contactref element="R39" pad="1"/>
<contactref element="C60" pad="1"/>
<contactref element="U2" pad="40"/>
</signal>
<signal name="SIGNAL2_DSUB">
<contactref element="D12" pad="3"/>
<contactref element="R38" pad="1"/>
<contactref element="C56" pad="1"/>
<contactref element="U2" pad="37"/>
</signal>
<signal name="LCD_RST">
<contactref element="DISPLAY" pad="3"/>
<contactref element="U2" pad="96"/>
</signal>
<signal name="LCD_BL">
<contactref element="DISPLAY" pad="4"/>
<contactref element="U2" pad="97"/>
</signal>
<signal name="CS_LCD">
<contactref element="DISPLAY" pad="10"/>
<contactref element="U2" pad="98"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="5"/>
<contactref element="X10" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="B1" pad="AC1"/>
<contactref element="L4" pad="CB"/>
</signal>
<signal name="N$33">
<contactref element="B1" pad="AC2"/>
<contactref element="L4" pad="CG"/>
</signal>
<signal name="N$2">
<contactref element="R18" pad="2"/>
<contactref element="LED3" pad="C@1"/>
</signal>
<signal name="N$35">
<contactref element="R19" pad="2"/>
<contactref element="LED1" pad="C@1"/>
</signal>
<signal name="CAN_VCC">
<contactref element="JP4" pad="2"/>
<contactref element="X3" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="AN_THERM">
<contactref element="TR1" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="U2" pad="42"/>
</signal>
<signal name="CS_LED">
<contactref element="JP6" pad="3"/>
<contactref element="U2" pad="140"/>
</signal>
<signal name="N$43">
<contactref element="IC6" pad="18"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="SIGNAL1">
<contactref element="S2" pad="1"/>
<contactref element="R24" pad="2"/>
<contactref element="U2" pad="56"/>
</signal>
<signal name="SIGNAL2">
<contactref element="S2" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="U2" pad="57"/>
</signal>
<signal name="SIGNAL4">
<contactref element="S2" pad="4"/>
<contactref element="R22" pad="2"/>
<contactref element="U2" pad="87"/>
</signal>
<signal name="SIGNAL8">
<contactref element="S2" pad="8"/>
<contactref element="R21" pad="2"/>
<contactref element="U2" pad="88"/>
</signal>
<signal name="LED_CATH_1">
<contactref element="LED2" pad="8"/>
<contactref element="LED2" pad="3"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="LED_DP">
<contactref element="LED2" pad="6"/>
<contactref element="LED4" pad="6"/>
<contactref element="LED5" pad="6"/>
<contactref element="LED6" pad="6"/>
<contactref element="IC6" pad="22"/>
</signal>
<signal name="LED_G">
<contactref element="LED2" pad="1"/>
<contactref element="LED4" pad="1"/>
<contactref element="LED5" pad="1"/>
<contactref element="LED6" pad="1"/>
<contactref element="IC6" pad="17"/>
</signal>
<signal name="LED_F">
<contactref element="LED2" pad="2"/>
<contactref element="LED4" pad="2"/>
<contactref element="LED5" pad="2"/>
<contactref element="LED6" pad="2"/>
<contactref element="IC6" pad="15"/>
</signal>
<signal name="LED_E">
<contactref element="LED2" pad="4"/>
<contactref element="LED4" pad="4"/>
<contactref element="LED5" pad="4"/>
<contactref element="LED6" pad="4"/>
<contactref element="IC6" pad="21"/>
</signal>
<signal name="LED_D">
<contactref element="LED2" pad="5"/>
<contactref element="LED4" pad="5"/>
<contactref element="LED5" pad="5"/>
<contactref element="LED6" pad="5"/>
<contactref element="IC6" pad="23"/>
</signal>
<signal name="LED_C">
<contactref element="LED2" pad="7"/>
<contactref element="LED4" pad="7"/>
<contactref element="LED5" pad="7"/>
<contactref element="LED6" pad="7"/>
<contactref element="IC6" pad="20"/>
</signal>
<signal name="LED_B">
<contactref element="LED2" pad="9"/>
<contactref element="LED4" pad="9"/>
<contactref element="LED5" pad="9"/>
<contactref element="LED6" pad="9"/>
<contactref element="IC6" pad="16"/>
</signal>
<signal name="LED_A">
<contactref element="LED2" pad="10"/>
<contactref element="LED4" pad="10"/>
<contactref element="LED5" pad="10"/>
<contactref element="LED6" pad="10"/>
<contactref element="IC6" pad="14"/>
</signal>
<signal name="LED_CATH_2">
<contactref element="LED4" pad="8"/>
<contactref element="LED4" pad="3"/>
<contactref element="IC6" pad="11"/>
</signal>
<signal name="LED_CATH_3">
<contactref element="LED5" pad="8"/>
<contactref element="LED5" pad="3"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="LED_CATH_4">
<contactref element="LED6" pad="8"/>
<contactref element="LED6" pad="3"/>
<contactref element="IC6" pad="7"/>
</signal>
<signal name="N$44">
<contactref element="JP6" pad="2"/>
<contactref element="IC6" pad="12"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="T1">
<contactref element="JP7" pad="2"/>
<contactref element="R26" pad="1"/>
<contactref element="C55" pad="1"/>
<contactref element="U2" pad="81"/>
</signal>
<signal name="T4">
<contactref element="R29" pad="1"/>
<contactref element="JP7" pad="8"/>
<contactref element="C52" pad="2"/>
<contactref element="U2" pad="86"/>
</signal>
<signal name="T3">
<contactref element="JP7" pad="6"/>
<contactref element="R28" pad="1"/>
<contactref element="C53" pad="2"/>
<contactref element="U2" pad="85"/>
</signal>
<signal name="T2">
<contactref element="R27" pad="1"/>
<contactref element="JP7" pad="4"/>
<contactref element="C54" pad="1"/>
<contactref element="U2" pad="82"/>
</signal>
<signal name="N$45">
<contactref element="LED7" pad="K"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="LED8" pad="K"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="X1" pad="9"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="X1" pad="4"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$79">
<contactref element="X1" pad="8"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$62">
<contactref element="X1" pad="COM_TERM"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="D3" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$2" pad="8"/>
<contactref element="U$2" pad="13"/>
<contactref element="U$2" pad="16"/>
<contactref element="U$1" pad="2"/>
<contactref element="C35" pad="-"/>
<contactref element="C34" pad="-"/>
<contactref element="C61" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="C50" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C30" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="C36" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="L2" pad="1"/>
<contactref element="X5" pad="2"/>
<contactref element="X6" pad="2"/>
<contactref element="X7" pad="2"/>
<contactref element="X8" pad="2"/>
<contactref element="X9" pad="2"/>
<contactref element="X10" pad="2"/>
<contactref element="X11" pad="2"/>
<contactref element="X12" pad="2"/>
<contactref element="D19" pad="A"/>
<contactref element="U2" pad="31"/>
<contactref element="C7" pad="-"/>
<contactref element="U5" pad="4"/>
<contactref element="C6" pad="-"/>
<contactref element="C49" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R35" pad="1"/>
<contactref element="X7" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R33" pad="1"/>
<contactref element="X6" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R34" pad="1"/>
<contactref element="X8" pad="1"/>
</signal>
<signal name="N$60">
<contactref element="R32" pad="1"/>
<contactref element="X5" pad="1"/>
</signal>
<signal name="N1">
<contactref element="DSUB_SCHNITTSTELLE" pad="SIGNAL_3"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="N2">
<contactref element="DSUB_SCHNITTSTELLE" pad="SIGNAL_2"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="N3">
<contactref element="DSUB_SCHNITTSTELLE" pad="SIGNAL_1"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="VCCIO">
<contactref element="U$2" pad="5"/>
<contactref element="C34" pad="+"/>
<contactref element="U$2" pad="6"/>
<contactref element="SJ2" pad="1"/>
<contactref element="D3" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C51" pad="1"/>
<contactref element="L8" pad="1"/>
<contactref element="D19" pad="C"/>
<contactref element="U5" pad="2"/>
<contactref element="C7" pad="+"/>
</signal>
<signal name="N$63">
<contactref element="X4" pad="1"/>
<contactref element="L4" pad="B"/>
</signal>
<signal name="N$78">
<contactref element="X4" pad="2"/>
<contactref element="L4" pad="PSG"/>
</signal>
<signal name="N$25">
<contactref element="IC4" pad="1"/>
<contactref element="C39" pad="2"/>
<contactref element="B1" pad="+"/>
<contactref element="IC5" pad="1"/>
<contactref element="C42" pad="+"/>
<contactref element="C43" pad="2"/>
</signal>
<signal name="CL1">
<contactref element="J2" pad="5"/>
<contactref element="L7" pad="2"/>
</signal>
<signal name="CH1">
<contactref element="J2" pad="4"/>
<contactref element="L7" pad="3"/>
</signal>
<signal name="CL21">
<contactref element="J1" pad="5"/>
<contactref element="L6" pad="2"/>
</signal>
<signal name="CH2">
<contactref element="J1" pad="4"/>
<contactref element="L6" pad="3"/>
</signal>
<signal name="CL3">
<contactref element="X3" pad="3"/>
<contactref element="L5" pad="2"/>
</signal>
<signal name="CH3">
<contactref element="X3" pad="2"/>
<contactref element="L5" pad="3"/>
</signal>
<signal name="N$85">
<contactref element="JP8" pad="1"/>
<contactref element="R40" pad="2"/>
</signal>
<signal name="LED1">
<contactref element="JP8" pad="2"/>
<contactref element="U2" pad="99"/>
</signal>
<signal name="LED2">
<contactref element="JP8" pad="4"/>
<contactref element="U2" pad="111"/>
</signal>
<signal name="LED3">
<contactref element="JP8" pad="6"/>
<contactref element="U2" pad="112"/>
</signal>
<signal name="LED4">
<contactref element="JP8" pad="8"/>
<contactref element="U2" pad="113"/>
</signal>
<signal name="N$90">
<contactref element="R43" pad="2"/>
<contactref element="JP8" pad="7"/>
</signal>
<signal name="N$91">
<contactref element="R42" pad="2"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="N$92">
<contactref element="R41" pad="2"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="TD_P">
<contactref element="U$3" pad="21"/>
<contactref element="R76" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="RMII_TX_EN">
<contactref element="U$3" pad="16"/>
<contactref element="U2" pad="126"/>
</signal>
<signal name="RMII_TXD0">
<contactref element="U$3" pad="17"/>
<contactref element="U2" pad="128"/>
</signal>
<signal name="RMII_MDC">
<contactref element="U$3" pad="13"/>
<contactref element="U2" pad="27"/>
</signal>
<signal name="NETR47_2">
<contactref element="U$3" pad="14"/>
<contactref element="R69" pad="1"/>
<contactref element="R44" pad="1"/>
</signal>
<signal name="RMII_MDIO">
<contactref element="U$3" pad="12"/>
<contactref element="R68" pad="1"/>
<contactref element="U2" pad="36"/>
</signal>
<signal name="NETR44_2">
<contactref element="U$3" pad="7"/>
<contactref element="R71" pad="2"/>
<contactref element="R50" pad="1"/>
</signal>
<signal name="NETR42_1">
<contactref element="U$3" pad="8"/>
<contactref element="R70" pad="2"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="NETR41_1">
<contactref element="U$3" pad="10"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="NETR39_2">
<contactref element="U$3" pad="11"/>
<contactref element="R72" pad="2"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="RMII_TXD1">
<contactref element="U$3" pad="18"/>
<contactref element="U2" pad="74"/>
</signal>
<signal name="NETC45_1">
<contactref element="U$3" pad="4"/>
<contactref element="C62" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="NETC44_2">
<contactref element="U$3" pad="1"/>
<contactref element="R73" pad="1"/>
<contactref element="R74" pad="1"/>
<contactref element="R76" pad="1"/>
<contactref element="C82" pad="1"/>
<contactref element="C83" pad="1"/>
<contactref element="C84" pad="1"/>
<contactref element="L10BEAD" pad="2"/>
<contactref element="T1" pad="2"/>
<contactref element="T1" pad="7"/>
<contactref element="U3" pad="5"/>
<contactref element="U$3" pad="19"/>
<contactref element="C76" pad="1"/>
<contactref element="C77" pad="1"/>
<contactref element="C65" pad="+"/>
<contactref element="R75" pad="1"/>
</signal>
<signal name="NETC43_1">
<contactref element="U$3" pad="5"/>
<contactref element="C63" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="NETC41_1">
<contactref element="U$3" pad="6"/>
<contactref element="C80" pad="1"/>
<contactref element="C81" pad="1"/>
</signal>
<signal name="N$93">
<contactref element="U$3" pad="24"/>
<contactref element="R64" pad="2"/>
</signal>
<signal name="NETR56_2">
<contactref element="R77" pad="1"/>
<contactref element="T1" pad="10"/>
</signal>
<signal name="NETC51_2">
<contactref element="R77" pad="2"/>
<contactref element="R78" pad="2"/>
<contactref element="R79" pad="2"/>
<contactref element="R80" pad="2"/>
<contactref element="C64" pad="1"/>
</signal>
<signal name="NETR57_2">
<contactref element="R78" pad="1"/>
<contactref element="T1" pad="15"/>
</signal>
<signal name="NETCN14_4">
<contactref element="R79" pad="1"/>
<contactref element="U$5" pad="4"/>
<contactref element="U$5" pad="5"/>
</signal>
<signal name="NETCN14_7">
<contactref element="R80" pad="1"/>
<contactref element="U$5" pad="7"/>
<contactref element="U$5" pad="8"/>
</signal>
<signal name="RMII_RXD1">
<contactref element="R50" pad="2"/>
<contactref element="U2" pad="45"/>
</signal>
<signal name="RMII_RXD0">
<contactref element="R51" pad="2"/>
<contactref element="U2" pad="44"/>
</signal>
<signal name="RMII_CRS_DV">
<contactref element="R52" pad="2"/>
<contactref element="U2" pad="43"/>
</signal>
<signal name="DIFF2_RD_N">
<contactref element="T1" pad="9"/>
<contactref element="U$5" pad="6"/>
</signal>
<signal name="DIFF2_RD_P">
<contactref element="T1" pad="11"/>
<contactref element="U$5" pad="3"/>
</signal>
<signal name="DIFF2_TD_N">
<contactref element="T1" pad="14"/>
<contactref element="U$5" pad="2"/>
</signal>
<signal name="DIFF2_TD_P">
<contactref element="T1" pad="16"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="RMII_REF_CLK">
<contactref element="R44" pad="2"/>
<contactref element="U2" pad="35"/>
</signal>
<signal name="USB_VBUS">
<contactref element="D20" pad="6"/>
<contactref element="R46" pad="2"/>
<contactref element="U4" pad="6"/>
<contactref element="C66" pad="+"/>
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="7"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="USB_ID">
<contactref element="D20" pad="1"/>
<contactref element="U2" pad="102"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="USB_POWERSWITCHON">
<contactref element="R45" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="U2" pad="91"/>
</signal>
<signal name="USB_OVERCURRENT">
<contactref element="U4" pad="5"/>
<contactref element="U2" pad="92"/>
</signal>
<signal name="N$50">
<contactref element="R46" pad="1"/>
<contactref element="U2" pad="101"/>
</signal>
<signal name="N$65">
<contactref element="U2" pad="9"/>
<contactref element="C68" pad="1"/>
<contactref element="Q2-RTC" pad="1"/>
</signal>
<signal name="N$66">
<contactref element="C67" pad="1"/>
<contactref element="Q2-RTC" pad="2"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="N$87">
<contactref element="U2" pad="33"/>
<contactref element="L10BEAD1" pad="2"/>
<contactref element="U2" pad="32"/>
<contactref element="C87" pad="1"/>
</signal>
<signal name="BUTTON2">
<contactref element="DSUB_SCHNITTSTELLE" pad="BUTTON_2"/>
<contactref element="D6" pad="3"/>
<contactref element="U2" pad="80"/>
</signal>
<signal name="BUTTON1">
<contactref element="DSUB_SCHNITTSTELLE" pad="BUTTON_1"/>
<contactref element="D7" pad="3"/>
<contactref element="U2" pad="79"/>
</signal>
<signal name="SPI1CS2">
<contactref element="DSUB_SCHNITTSTELLE" pad="SPI1_CS2"/>
<contactref element="D8" pad="3"/>
<contactref element="U2" pad="78"/>
</signal>
<signal name="N$94">
<contactref element="U2" pad="106"/>
<contactref element="C90" pad="1"/>
</signal>
<signal name="N$95">
<contactref element="U2" pad="71"/>
<contactref element="C89" pad="1"/>
</signal>
<signal name="N$97">
<contactref element="U2" pad="138"/>
<contactref element="R53" pad="1"/>
</signal>
<signal name="N$98">
<contactref element="U2" pad="143"/>
<contactref element="JMP1" pad="2"/>
</signal>
<signal name="SIGNAL4_DSUB">
<contactref element="U2" pad="77"/>
<contactref element="DSUB_SCHNITTSTELLE" pad="SIGNAL_4"/>
<contactref element="D10" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="JTAG" pad="19"/>
<contactref element="R47" pad="2"/>
</signal>
<signal name="VREF">
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="JTAG" pad="11"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="JTAG" pad="17"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="USB_P">
<contactref element="D20" pad="3"/>
<contactref element="U2" pad="104"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="TD_N">
<contactref element="U$3" pad="20"/>
<contactref element="R75" pad="2"/>
<contactref element="T1" pad="3"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="RD_P">
<contactref element="U$3" pad="23"/>
<contactref element="R74" pad="2"/>
<contactref element="T1" pad="6"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="RD_N">
<contactref element="U$3" pad="22"/>
<contactref element="R73" pad="2"/>
<contactref element="T1" pad="8"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="USB_N">
<contactref element="D20" pad="4"/>
<contactref element="U2" pad="103"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="23"/>
<contactref element="8MHZ" pad="3"/>
</signal>
<signal name="N$34">
<contactref element="U2" pad="2"/>
<contactref element="SV5" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="U2" pad="3"/>
<contactref element="SV5" pad="3"/>
</signal>
<signal name="N$37">
<contactref element="U2" pad="4"/>
<contactref element="SV5" pad="4"/>
</signal>
<signal name="N$38">
<contactref element="U2" pad="5"/>
<contactref element="SV5" pad="5"/>
</signal>
<signal name="N$39">
<contactref element="U2" pad="1"/>
<contactref element="SV5" pad="1"/>
</signal>
<signal name="N$59">
<contactref element="U2" pad="7"/>
<contactref element="SV5" pad="6"/>
</signal>
<signal name="N$41">
<contactref element="U2" pad="10"/>
<contactref element="SV5" pad="7"/>
</signal>
<signal name="N$53">
<contactref element="U2" pad="11"/>
<contactref element="SV5" pad="8"/>
</signal>
<signal name="N$54">
<contactref element="U2" pad="12"/>
<contactref element="SV5" pad="9"/>
</signal>
<signal name="N$52">
<contactref element="U2" pad="13"/>
<contactref element="SV5" pad="10"/>
</signal>
<signal name="N$40">
<contactref element="U2" pad="14"/>
<contactref element="SV5" pad="11"/>
</signal>
<signal name="N$42">
<contactref element="U2" pad="15"/>
<contactref element="SV5" pad="12"/>
</signal>
<signal name="N$55">
<contactref element="U2" pad="18"/>
<contactref element="SV5" pad="13"/>
</signal>
<signal name="N$56">
<contactref element="U2" pad="19"/>
<contactref element="SV5" pad="14"/>
</signal>
<signal name="N$48">
<contactref element="U2" pad="20"/>
<contactref element="SV5" pad="15"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="28"/>
<contactref element="SV5" pad="20"/>
</signal>
<signal name="N$10">
<contactref element="U2" pad="29"/>
<contactref element="SV5" pad="19"/>
</signal>
<signal name="N$49">
<contactref element="U2" pad="26"/>
<contactref element="SV5" pad="17"/>
</signal>
<signal name="N$51">
<contactref element="U2" pad="22"/>
<contactref element="SV5" pad="18"/>
</signal>
<signal name="N$57">
<contactref element="U2" pad="21"/>
<contactref element="SV5" pad="16"/>
</signal>
<signal name="N$61">
<contactref element="U$3" pad="3"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="N$64">
<contactref element="U$3" pad="2"/>
<contactref element="R54" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
